UIL Theatrical Design Contest

Students participating in SET DESIGN should design their set for production on the Leage High School stage . The measurements of that space follow:

LEAGUE HIGH SCHOOL STAGE DIMENSIONS

Type stage: Proscenium

Proscenium Width: 36’0”

Apron Depth: 4’0”

Curtain Line to Back Wall: 36’0”

Proscenium Height: 20’0”

Designers choice of Legs, Mid or Back Travelers, Scrims, or drops may be placed on the following batens as needed:

Position of Batens (from Curtain Line)

Set 1 2’0”

Set 2 8’0”

Set 3 14’0”

Set 4 20’0”

Set 5 26’0”

Set 6 32’0”

Sample Drawings are available on the website, but students should do their own drawing or create their own drawing in CAD using these measurements. This stage will fit on the required 11x17 plate size if drawn in 1’0” =0’ 3/16” scale.

Remember to use USITT Standards as a reference for correct drafting style and to include the ¼” border and Title Block on your drawings. These guidelines can be found on-line and in books. A helpful site that shows examples is:

http://department.monm.edu/theatre/Rankin/Classes/THEA181/draftingusittstandards2.pdf